SHIPS PARTICULAR
====================== VESSEL NAME : East Wind I	EX " NORDIC BULKER 2 “
TYPE : BULK CARRIER -Single Deck	FLAG : PANAMA	BUILT : 10/02 AT IMABARI SHIPBUILDING CO LTD - IMABARI EH (IMABARI , JPN
P.O.R :	Panama
M.M.S.I .NO : 372077000	CALL SIGN : 3FCK9	IMO NO. : 9278973	TLX NO. :
TLX NO. : Inmarsat C No. :
Vsl’s Fleet  :
CLASS :  B.V.	OFFICAL NO : Panama re.g No.: 53727-PEXT
P&I CLUB : MS. Amlin Marine N.V.
OWNERS : EAST WIND SHIPPING CO.  - Republic of the Marshal Islands –
Reg. No. : 108454

[bookmark: _GoBack]

DIMENTIONS : L.O.A 169.26 M	BEAM: 27.20 M	L.B.P M : 160.4 m	DEPTH: 13.60 M TONNAGE :	INTRNAL		SUEZ		PANAMA
GRT	16966 tons	17486.78 mts	PC / UMS
NRT		10498 mts		15995.56 mts	14197 mts Hull No. = m	= insured Value : 5 500 000 $DEAD WEIGHT  28,458 tons	LIGHT WEIGHT = 6,131LT	T.P.C = T /  F.W.A  MM
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Logs Fitted	= 5 Holds / 5 Hatches
	HOLDS CAPACITY
	GRAIN M3
	BALE
	HOLDS DIMENSION
	
	
	

	HOLD NO.1
	5319.76 cbm
	5016.06 cbm
	
	L
	W
	H

	HOLD NO.2
	8236.33 cbm
	7480.01 cbm
	HOLD NO.1
	22.4
	F:8.70-A 12.20
	12.20m

	HOLD NO.3
	8260.63 cbm
	7882.90 cbm
	HOLD NO.2
	26.5
	F:23.5 –A 26.8
	12.20 m

	HOLD NO.4
	8298.00 cbm
	7878.90 cbm
	HOLD NO.3
	26.5
	26.8
	12.20 m

	HOLD No. 5
	7408.29 cbm
	7140.58 cbm
	HOLD NO.4
	26.5
	F:26.8 –A 25.2
	12.20 m

	TOTAL
	37523.01CBM
	35762.45CBM
	HOLD NO.5
	26.5
	F:25.0 – A 12.2
	12.20 m



	HATCH SIZE
	LENGTH
	BREADTH

	HATCH NO. : 1
	13.60  M
	16.00 M

	HATCH NO. : 2 + 3 + 4 + 5
	19.20 M
	17.60 M

	HATCH COVER TYPE : FOLDING TYPE Steel =OPERATED HYDAULICALLY –
Hatch Cover Strenght : 3300 ts / Sq.M

	GEAR TYPE
	4 CRANES X 30.5 mts Electro Hydraulic	=  SWL / outreach r
(manufacturer=
Located  Center Line

	
	BWTS IS FITTED

	Deck Strengths : Upper Deck Side 4.100 t/ Sq.M	-  Cross Deck: 3.300 T/Sq. M
Tank Top dimensions ( L X W ) in Meters : Hold No. 1 : 22.4 X B (fwd) 8.70 X aft 12.20
Hold No. 2 : 26.5 X B (fwd) 23.50 X 26.8
Hold No. 3 : 26.5 X 26.8
Hold No. 4 : 26.5 X B (fwd) 26.8 X ( aft ) 25.2
Hold No. 5 : 26.5 X B (fwd) 25.0 X aft 12.0

	



	MAIN ENGINE
	B&W 6S42MC
Engine Cannot be operated at Critical RPM

	
	

	SPEED / CONSUMPTION
	BALLAST		ABT 13K ON ABT 19 MT VLSIFO + 0.1 MT MGO ABT 12K ON ABT 16 MT VLSIFO + 0.1 MT MGO ABT 11K ON ABT 14.5 MT VLSIFO + 0.1MT MGO

LADEN		ABT 12.5 K ON ABT 20.0MT VLSIFO + 0.1 MT MGO/MDO ABT 12.0 K ON ABT 19.0MT VLSIFO + 0.1 MT MGO/MDO ABT 11.0 K ON ABT 17.0MT VLSIFO + 0.1MT MGO/MDO
IN PORT CONSUMPTION:
IDLE	ABT 2.5MT VLSIFO + 0.1MT MGO/MDO T/Day WORKING   ABT 5.5MT VLSIFO + 0.1 MT MGO/MDO T/Day

	AUXILIARIES
	No. & capacity of generators =

	
	A60 bulk head insulation + Australian ladders fitted in all holds

	
	NEXT SPECIAL SURVEY: 2022-10-03 NEXT DRY DOCK: 2022-10-03

	Tank Capacities
	VLS IFO	abt 1057 Cum
LSMGO	abt 0117 cum Ballast water abt 8312.35 cum Fresh Water abt 0293 cum
Constant excluding Fresh Water : 223 mts



