“ MV  MATTEO BR ”

SHIP BASIC 
YARD                    		ZHEJIANG AOLI SHIPBUILDING CO LTD - CHINA             
DATE OF KEEL LAID       	26 AUGUST 2008  
DATE OF DELIVERY/BUILT  	26 JUNE 2010
TYPE OF VESSEL          		GENERAL CARGO 
FLAG                    		ITALIAN  
PORT OF REGISTRY        	NAPOLI
CLASSIFICATION          		RINA CLASS REGISTER 
TRADING                 		UNRESTRICTED AREA 
IMO NUMBER              	9556844
CLASS NR                		88414
H+M INSURANCE COMPANY   	GENERALI
H+M VALUE               		20 MIL USD 
PANDI                   		STANDARD P&I CLUB
 
DIMENSION AND MAIN DATA 
LENGTH OVERALL          	157,00
LENGTH BETWEEN PP       	149,80
BREADTH MOULDED         	24,80
DEPTH MOULDED           	13,70
HEIGHT ABOVE KEEL       	40,00
GT/NT                   		15545/8149
SUEZ GT/NT              		15699,78/14766,01
DESIGNED DRAFT          	9,80
DWT                     		25035
TPC SUMMER DWT          	35,00 
DISTANCE FROM WATER LINE TO TOP OF HATCHCOMING ABT 6.00 LOADED
DISTANCE FROM WATER LINE TO TOP OF HATCHCOMING ABT 10.60 BALLAST  
DISTANCE FROM BOW TO BEGINNING FORE BULKHEAD HOLD NR 1 :  16,00
DISTANCE FROM STERN TO END OF AFT BULKHEAD   HOLD NR 4 :  31,20
 
 
HOLD/HATCHES 
NUMBER OF HO/HA        	 4/4  
 
DIMENSION 
HATCH NR 1              		17,60 X 14,00           M  
HATCH NR 2              		19,20 X 17,20           M 
HATCH NR 3              		19,20 X 17,20           M 
HATCH NR 4              		19,20 X 17,20           M
HOLD NR 1               		26 X 22 X 14            M
HOLD NR 2               		28 X 22 X 14            M
HOLD NR 3               		28 X 22 X 14            M
HOLD NR 4               		27 X 22 X 14            M
HEIGHT OF H/COAMING     	2,00 
TYPE OF HATCHES         	FOLDING 
                 
HOLD/TANK CAPACITY ABT 
CARGO HOLD ABT 		(GRAIN / BALE): 
NR 1                    		245599 / 240687 CBFT 
NR 2                    		286908 / 281170 CBFT
NR 3                    		286908 / 281170 CBFT
NR 4                    		272286 / 266841 CBFT
TOTAL                   		1091701 CBFT GRAIN 
                        		1069868 CBFT BALE 
BALLAST                 		7256,40  CBM
F.WATER                		519.50   CBM
FUEL OIL                		891        CBM
DIESEL OIL              		215        CBM
LUB OIL                 		77,80    CBM
OTHER TANKS             		104,10   CBM
 
CARGO GEAR 
TYPE                    		3 CRANES 
SWL                     		30,5 MT EACH
SITUATED                		CENTRAL 
RADIUS MIN/MAX          	4,5/24 M


 
DECK STREINGHT 
TANK TOP                		18   MT / SQM
HATCH – COVERS          	1,75 MT / SQM
 
SPEED /CONSUMPTION
SPEED                   		ABT 11.5 KN / ABT 15 TS ULSFO 
                        		ISO 8217/2024  + 0.8TS MGO MAX 0.1 SULF DMA SPEC 
BSS MAX BEAUFORT 4 NO SWELL AND NO ADVERSE CURRENTS 
                        
IN PORT W/OUT GEAR      	0.8   MT GASOIL 
[bookmark: _GoBack]IN PORT WITH GEAR       	2.4   MT GASOIL  
 
VSL BURN GASOIL ON RESTRICTED AREA / RIVER / CANAL AND ON PORT MANUVRING 
VSL MUST USE MGO LOW SULFHUR FOR EUROPEAN PORTS AND SECA AREA 
 
VENTILATION 
HOLD                    		MECHANICAL , 6 AIR CHANGES PER HOUR   
 
ADDITIONAL INFO 
APP A/B/C FITTED 
CO2 FITTED IN CARGO HOLDS 
LOADING COMPUTER
ISM/ISPS CERTIFIED 
GRAIN FITTED 

ALL DETAILS TO BE ABOUT AND GIVEN WITHOUT GUARANTEE
 

